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Description:Vegetable Base
Appearance:Liquid
Product Summery:FAC producted through hydrolysis, distillation and other processes based on soyabean oil.
Packing:20MT net/Flexitank
	Item
	Test Method
	Qualified Value

	Appearance
	Visual
	Conform

	Colour(Fe-Co)
	GB/T1722
	5 Max

	Acid Value(mgKOH/g)
	GB/T9104.3
	185-210

	Iodine Value(gl2/100g)
	GB/T9104.1
	144 Min

	Saponification Value(mgKOH/g)
	GB/T9104.2
	186-211

	Solidifying Point(℃)
	GB/T510
	-12 Max

	Cloud Point(℃)
	ASTM D2500b
	-8 Max

	Saturated Fatty Acids(%)
	GB/T17376
	2.5 Max

	Moisture(%)
	GB/T9104.6
	0.3 Max
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